**System View of Threads**

1. **User-Level Threads**:
   * **What They Are**: Threads created and managed by application software (like in a program or app).
   * **Role**: Allow the application to perform multiple tasks at once.
   * **Example**: In a web browser, separate threads might handle different tabs.
2. **Kernel-Level Threads**:
   * **What They Are**: Threads managed by the operating system (OS).
   * **Role**: The OS schedules these threads and handles their execution.
   * **Example**: The OS might schedule threads for a word processor to ensure smooth performance.
3. **Hardware Threads**:
   * **What They Are**: Threads as seen by the CPU or hardware.
   * **Role**: Hardware can run multiple threads simultaneously if it supports features like hyper-threading.
   * **Example**: A CPU core with hyper-threading can handle two threads at the same time.

**Multi-threading on Single-Core versus MultiCore Platforms**

**Single-Core Platforms**


On a single-core platform, only one thread can execute at a time. Here’s how multi-threading works:


* **Context Switching:** When multiple threads are present, the operating system (OS) performs context switching, which involves saving the state of the current thread and loading the state of the next thread. This switching happens so quickly that it gives the illusion of simultaneous execution.
* **Overhead:** Context switching introduces overhead because the CPU must save and restore thread states. Excessive switching can reduce performance, especially if threads frequently need to switch.
* **Concurrency vs. Parallelism:** On a single-core system, you achieve concurrency (managing multiple threads in an overlapping time frame) but not parallelism (executing threads at the same time).

**Multi-Core Platforms**

On multi-core platforms, each core can execute its thread simultaneously, which changes the dynamics:

* **True Parallelism:** Multiple threads can be executed truly in parallel across different cores. This can lead to significant performance improvements for multi-threaded applications as threads do not need to wait for each other to complete.
* **Load Balancing:** The OS or runtime environment must effectively manage thread distribution across cores to ensure balanced load and avoid scenarios where some cores are overloaded while others are idle.
* **Scalability:** Multi-core systems typically handle increases in the number of threads better, as each core can handle separate threads independently. However, performance improvements can vary depending on how well the application’s workload can be divided among threads.

****



|  |  |  |
| --- | --- | --- |
| **Aspect** | Single-Core Platforms | Multi-Core Platforms |
| Execution | Only one thread can execute at a time. | Multiple threads can execute simultaneously. |
| Context Switching | Involves saving and loading thread states, creating overhead. | Less context switching; threads run in parallel across cores. |
| Overhead | High overhead due to frequent context switching. | Lower overhead as threads run simultaneously. |
| Concurrency | Achieves concurrency by managing multiple threads over time. | Achieves true parallelism with simultaneous thread execution. |
| Parallelism | Does not achieve parallelism (all threads are not running at the same time). | Achieves parallelism (threads can run at the same time on different cores). |
| Load Balancing | Not applicable (only one core). | Must balance threads across multiple cores. |
| Scalability | Limited by a single core’s capacity. | Better scalability with more cores handling more threads. |

**Parallel Computing Platform:**

A parallel computing platform is a system that enables multiple processors or cores to work together on a task simultaneously, improving computational speed and efficiency. In parallel computing, tasks are divided into smaller subtasks that can be processed concurrently, leading to faster execution times.

**Key Concepts:**

* **Parallelism:** The practice of running multiple computations at the same time to speed up processing.
* **Distributed Memory Systems:** Each processor has its own memory, and processors communicate via a network.
* **Shared Memory Systems:** All processors share a common memory space, allowing direct access to data by any processor.

**Gustafson's Law**

**Gustafson's Law** is a model used in computer architecture to evaluate the potential speedup of a task that benefits from parallel computing.

Unlike Amdahl's Law, which focuses on a fixed problem size, Gustafson's Law considers increasing problem size as the number of processors increases.

Gustafson’s Law suggests that the speedup of a parallel computing system depends on the problem size and the number of processors used. Unlike Amdahl’s Law, which focuses on the fraction of the program that can be parallelized, Gustafson’s Law focuses on how increasing the problem size can lead to increased performance with more processors.

**Key points:**

* **Problem size scales with processor count:** As the number of processors grows, the problem size is also increased to maintain a constant execution time.
* **Focuses on large-scale problems:** Gustafson's Law is particularly relevant for problems that can be significantly expanded to take advantage of additional processors.
* **Linear speedup:** Under ideal conditions, Gustafson's Law suggests that a linear speedup can be achieved as the number of processors increases.

**Formula:**

* **Speedup = s + (1-s) \* N**
  + s: Sequential fraction of the problem
  + N: Number of processors

**challenges associated with using threads**

 **Synchronization**:

* **Definition**: Coordinating the activities of two or more threads.
* **Example**: One thread waits for another to complete a task before it proceeds.
* **Challenge**: Ensuring threads operate in a coordinated manner to avoid conflicts and data corruption.

 **Communication**:

* **Definition**: Managing the exchange of data between threads.
* **Issues**:
  + **Bandwidth**: The amount of data that can be transmitted between threads.
  + **Latency**: The time delay in data transfer between threads.
* **Challenge**: Efficiently exchanging data to minimize delays and ensure smooth operation.

 **Load Balancing**:

* **Definition**: Distributing work evenly across multiple threads.
* **Challenge**: Ensuring that all threads have a roughly equal amount of work to avoid bottlenecks and underutilization of resources.

 **Scalability**:

* **Definition**: Making efficient use of a larger number of threads on more-capable systems.
* **Example**: Adapting a program optimized for four processor cores to efficiently use eight processor cores.
* **Challenge**: Ensuring that performance improvements scale with the addition of more threads or processing cores.

**Parallel Programming Patterns**

## Task-level Parallelism Pattern

* + Decompose problem into independent tasks
  + Remove dependencies between tasks or separate dependencies using replication
  + Suitable for embarrassingly parallel problems and replicated data problems.

# Divide and Conquer Pattern

* Divide problem into parallel sub-problems
* Solve each sub-problem independently
* Aggregate results into final solution
* Suitable for sequential algorithms like merge sort
* Good load balancing and locality

# Geometric Decomposition Pattern

* Focuses on parallelizing the data structures used in the problem by dividing the data into chunks.
* Each thread is assigned a portion of the data to process, typically based on geometric or spatial properties.
* Problems such as heat flow and wave propagation.

# Pipeline Pattern

* Breaks down computation into a series of stages, similar to an assembly line.
* A sequence of stages, where the output of one stage is the input to the next. Different stages can work in parallel on different pieces of data.
* Each thread works on a different stage simultaneously.

# Wavefront Pattern

* Processes data elements along a diagonal in a two-dimensional grid.
* Each element depends on previous elements being processed
* Tasks are executed in a diagonal wavefront pattern. Computation starts at one corner of the grid and progresses diagonally. All tasks within the same diagonal can be executed in parallel.
* Minimizes idle time for threads.
* Focuses on load balancing.

**Deadlock**

A deadlock is a situation in which two or more threads are blocked indefinitely, each waiting for the other to release a resource. This creates a circular dependency, where each thread is waiting for the other to complete its task, resulting in a deadlock.

**Conditions for Deadlock**

For a deadlock to occur, the following four conditions must be met:

1. **Mutual Exclusion**: At least one resource must be held in a non-sharable mode. meaning only one process can use the resource at any given time. If another process requests that resource, it must wait until the resource is released.
2. **Hold and Wait**: One thread must be holding a resource and waiting for another resource, which is held by another thread.
3. **No Preemption**: Resources cannot be forcibly taken away from a process that is holding it.
4. **Circular Wait**: A circular wait must exist, where each thread is waiting for another thread to release a resource.

 **Prevention**:

* **Avoiding Mutual Exclusion**: Make resources shareable where possible. If multiple processes can use a resource simultaneously, deadlock is less likely.
* **Preventing Hold and Wait**: Require processes to request all needed resources at once, or release all resources before requesting new ones.
* **Allowing Preemption**: Allow the system to forcibly take resources from processes if needed.
* **Avoiding Circular Wait**: Impose a resource allocation order to prevent circular wait conditions.

 **Avoidance**:

* **Dynamic Allocation**: Use algorithms like the Banker's Algorithm to allocate resources in a way that avoids deadlock situations.
* **Resource Allocation Graph**: Maintain a graph to track resources and their allocation to prevent circular wait.

|  |  |  |
| --- | --- | --- |
| Characteristics | Thread | Core |
| Definition | A separate flow of execution within a process | A physical processing unit in a CPU |
| Resource Sharing | Shares memory space and resources with parent process | Has its own dedicated resources (e.g. registers, cache) |
| Creation/ Destruction | Lightweight, created and destroyed quickly | Heavyweight, requires significant system resources |
| Context Switching | Fast context switching between threads | Slower context switching between cores |
| Parallelism | Multiple threads can run concurrently, but may not execute in parallel | Multiple cores can execute instructions in parallel |
| Scheduling | Scheduled by the operating system | Scheduled by the CPU's scheduler |
| Memory Access | Shares memory with parent process | Has its own dedicated memory access |
| Processing Power | Utilizes a portion of the core's processing power | Has its own dedicated processing power |
| Scalability | Can be scaled up to a certain limit, but may lead to thread thrashing | Can be scaled up to increase overall processing power |

**Synchronization Primitives**

Synchronization primitives are mechanisms used to coordinate the execution of concurrent processes or threads, ensuring that they access shared resources in a controlled manner to prevent conflicts and maintain consistency. Here are some common synchronization primitives:

**Common Synchronization Primitives:**

1. **Mutex (Mutual Exclusion)**:
   * **Definition**: A lock that allows only one thread to access a resource at a time.
   * **Usage**: Protects critical sections of code where shared resources are accessed.
   * **Operation**: A thread locks the mutex before accessing the shared resource and unlocks it when done. If another thread tries to lock it while it's already locked, it will be blocked until the mutex is unlocked.
   * **Challenges Addressed**:

* **Race Conditions**: Mutexes prevent race conditions by ensuring exclusive access to shared resources.
* **Deadlock**: Properly designed mutexes can prevent or reduce the likelihood of deadlocks by ensuring that resources are acquired in a consistent order.

1. **Semaphore**:
   * **Definition**: A counter-based synchronization primitive that controls access to resources.
   * **Types**:
     + **Counting Semaphore**: Allows a set number of threads to access a resource. The counter is incremented when a resource is released and decremented when a resource is acquired.
     + **Binary Semaphore**: Similar to a mutex, but does not enforce mutual exclusion; it allows only binary (0 or 1) values.
   * **Operation**: Threads wait (decrement) or signal (increment) the semaphore to acquire or release resources.

* **Challenges Addressed**:
* **Resource Contention**: Counting semaphores manage multiple threads' access to a finite number of resources.
* **Deadlock**: Proper use of semaphores can avoid circular wait conditions by ensuring that resources are acquired and released in a controlled manner.

1. **Condition Variable**:

* **Definition**: Used to block a thread until a specific condition is met.
* **Usage**: Often used with mutexes to allow threads to wait for certain conditions before continuing execution.
* **Operation**: A thread waits on a condition variable while holding a mutex. When another thread changes the state and signals the condition variable, the waiting thread is notified and can proceed.
* **Challenges Addressed**:
* **Thread Coordination**: Allows threads to efficiently wait for changes in shared data.
* **Spurious Wakeups**: Ensures threads only proceed when the desired condition is met, not just upon waking.

1. **Spin Lock**:

* **Definition**: The spin lock is a locking system mechanism. It allows a thread to acquire it to simply wait in loop until the lock is available .
* **Usage**: Effective for scenarios with short lock durations and low contention, where threads frequently acquire and release the lock quickly.
* **Operation**: A thread repeatedly checks (spins) to see if the lock is available. If the lock is held by another thread, the spinning thread continues to check until it can acquire the locks.
* **Challenges Addressed**:
* **Thread Contention**: Manages access to shared resources by ensuring that only one thread can access the resource at a time.
* **Synchronization Overhead**: Reduces the overhead of more complex synchronization methods when locks are held briefly.

1. **Monitor**:

* **Definition**: An abstraction that combines mutexes and condition variables.
* **Usage** Provides a way to ensure mutual exclusion and condition synchronization within an object or module.
* **Operation**: A monitor encapsulates shared data and methods, ensuring that only one thread can execute a method at a time. It provides condition variables to wait and signal conditions.
* **Challenges Addressed**:
* **Encapsulation**: Provides a cleaner way to manage synchronization by combining resource access control and condition synchronization.
* **Deadlock**: Properly implemented monitors reduce the risk of deadlocks by encapsulating locking mechanisms within an object.

1. **Read/Write Lock**:
   * **Definition**: Allows multiple readers or a single writer to access a resource, but not both simultaneously.
   * **Types**:
     + Shared (Read) Lock: Multiple threads can hold shared locks if they only need to read the resource.
     + Exclusive (Write) Lock: Only one thread can hold an exclusive lock, and no other thread can hold a shared or exclusive lock simultaneously.
   * **Operation**: Optimizes access for scenarios with many readers and fewer writers.
   * **Challenges Addressed**:
   * **Performance**: Improves efficiency by allowing concurrent reads while ensuring exclusive access for writes.
   * **Contention**: Balances the need for access to shared resources with the need to maintain data consistency.
2. **Atomic Operations**:

* **Definition**: Low-level operations that are completed as a single, indivisible step.
* **Usage** :Used for simple synchronization tasks like incrementing a counter or setting a flag..
* **Operation**: Ensures that operations are performed without interference from other threads, typically implemented in hardware.
* **Challenges Addressed**:
* **Race Conditions**: Ensures that operations on shared data are performed atomically, preventing conflicts.

**Challenges in Managing Simultaneous Activities (Concurrent Programming)**

Managing simultaneous activities in programming, known as concurrent programming, involves several challenges:

1. **Synchronization:** Ensuring multiple threads access shared resources safely using locks or semaphores to prevent data corruption.
2. **Race Conditions:** Occur when threads access shared resources at the same time, leading to unpredictable outcomes.
3. **Deadlocks:** Happen when threads wait indefinitely for each other to release resources, causing the program to freeze.
4. **Starvation:** A thread can’t use resources because other threads are using them all, which makes everything run slower.
5. **Livelocks:** Similar to deadlocks, but threads keep running without making progress.
6. **Cache Coherence:** In multi-core systems, keeping caches consistent across cores when accessing shared data is challenging.
7. **Scalability:** Managing more threads increases complexity and can lead to performance issues.
8. **Debugging & Testing:** Hard to reproduce errors in concurrent programs due to unpredictable thread execution.
9. **Platform Dependencies:** Concurrent code may behave differently on different platforms, affecting portability.
10. **Resource Constraints:** Requires careful management of CPU, memory, and I/O resources.
11. **Real-time Constraints:** Meeting timing requirements in systems with limited resources is difficult.

**Flow Control-based Concepts**

**Fence:**

* It ensures that all memory operations specified before the fence instruction are completed before any operations after the fence are started.
* Fence instructions can be error-prone if not used correctly and can affect performance due to their overhead.
* When the computer hits the fence, it has to wait until all the earlier tasks are done before it can start the next ones.
* This helps in keeping memory operations in the right order, but using fences can slow things down. So, it's often better to let the computer’s tools handle fences automatically instead of doing it yourself.

**Barrier:**

* A barrier is a synchronization mechanism that ensures that all threads in a group reach a certain point in their execution before any thread can proceed beyond that point.
* When a thread reaches a barrier, it must wait until all other threads in the same group have also reached the barrier. Only then can all the threads continue execution beyond the barrier.
* This keeps threads synchronized, but if not managed well, it can lead to delays. So, it's important to plan how tasks are divided up to avoid performance issues.

|  |  |  |
| --- | --- | --- |
| Aspect | Fence | Barrier |
| Purpose | Ensures memory operations are completed in the correct order. | Synchronizes multiple threads to reach the same point before proceeding. |
| How It Works | Acts as a checkpoint, ensuring all prior memory operations are finished before new ones start. | Acts as a meeting point where all threads wait until they all arrive before moving forward. |
| Impact | Affects memory ordering, not thread execution. | Affects both memory ordering and thread execution. |
| Usage | Critical sections, memory-intensive operations. | Parallel loops, coordinated execution. |
| Example | Ensures a write operation is complete before a subsequent read operation starts. | Ensures all threads complete their tasks in a loop before any proceed to the next iteration. |

**Problems with semaphores, locks, and condition variables**

**Semaphores**

* **Complexity**: Difficult to understand and implement correctly.
* **Deadlocks**: If not used carefully, semaphores can lead to deadlocks, where multiple threads are blocked waiting for resources held by each other.
* **Priority Inversion**: Low-priority threads holding semaphores can delay high-priority threads.

**Locks**

* **Deadlocks**: Can happen if threads acquire multiple locks in different orders.
* **Priority Inversion**: Similar issue where low-priority threads block high-priority ones.
* **Starvation**: Some threads may never get a chance to acquire the lock.
* **Deadlock Recovery**: Difficult to recover from deadlocks if they occur.

**Condition Variables**

* **Spurious Wakeups**: Threads might wake up without the condition being met.
* **Lost Wakeups**: If a signal is sent before a thread starts waiting, it might miss the wakeup signal.
* **Race Conditions**: Requires careful management of mutexes to avoid issues.
* **Complexity**: Managing both the condition variable and mutex is error-prone.

**Parallel Programming**

**Parallel programming** is a method of computing in which multiple processes or threads execute simultaneously to solve a problem or perform a task more efficiently. It involves dividing a large task into smaller sub-tasks that can be processed concurrently, often leveraging multiple processors or cores. Parallel programming is essential for taking full advantage of modern multi-core and multi-processor systems.

**Need Of Parallel Programming**

1. **Performance Improvement**:
   * **Speed**: Reduces execution time by processing multiple tasks simultaneously.
   * **Scalability**: Handles larger or more complex problems efficiently as core count increases.
2. **Efficient Resource Utilization**:
   * **Multi-Core Systems**: Utilizes the processing power of multiple cores effectively.
3. **Handling Large Data Sets**:
   * **Data Processing**: Allows efficient handling of large volumes of data by processing chunks in parallel.
4. **Complex Problem Solving**:
   * **Algorithms**: Enables efficient implementation of parallelizable algorithms.
5. **Responsiveness**:
   * **User Experience**: Maintains responsiveness in interactive applications by managing multiple tasks concurrently.
6. **Reducing Latency**:
   * **Real-Time Systems**: Minimizes response times by processing tasks concurrently.
7. **Energy Efficiency**:
   * **Power Usage**: Can lead to reduced power consumption by completing tasks more quickly.
8. **Modern Hardware**:
   * **Hardware Design**: Exploits the capabilities of multi-core and multi-processor systems for optimal performance.

|  |  |  |
| --- | --- | --- |
| Feature | Mutex | Lock |
| Implementation | Binary semaphore with atomic variable and waiting queue | Various synchronization primitives (semaphores, monitors, atomic variables |
| Behavior | Strict mutual exclusion, only one thread can acquire at a time | Can be implemented with various behaviors (exclusive, shared, read-write) |
| Thread Safety | Keeps threads safe by stopping them from using the same resource at the same time. | Also keeps threads safe by controlling resource access. |
| Usage | Used for short tasks, fine-grained synchronization (critical sections) | Used for longer tasks, coarser-grained synchronization (data structures, complex operations) |
| Performance | Lightweight and efficient | Can be heavyweight and slower, depending on implementation |
| Complexity | Simpler to implement and use | More complex to implement and use, with additional features (e.g., lock timeouts, priority inheritance) |
| Acquisition | Only one thread can acquire at a time | Can be acquired by multiple threads (depending on implementation) |
| Release | Released by the thread that acquired it | Released by the thread that acquired it, or by a separate thread (depending on |

|  |  |  |
| --- | --- | --- |
| Aspect | Deadlock | Livelock |
| Definition | A situation where two or more threads are blocked, waiting for each other to release resources, leading to a standstill. | A situation where threads are not blocked but continuously change their states without making progress. |
| State of Threads | Threads are stuck and do not proceed. | Threads are active but cannot make progress. |
| Cause | Circular wait and resource holding lead to a deadlock. | Threads repeatedly react to each other, preventing progress. |
| Resolution | Requires external intervention or timeout to resolve. | Often resolves automatically but might require external intervention. |
| Detection | Easier to detect because the system is stalled. | Harder to detect as the system appears active but isn't making real progress. |
| Examples | Two threads waiting for each other to release a lock. | Two threads continuously yielding to each other without completing their tasks |

**Threading API’s for Microsoft .NET Framework.**

The Microsoft .NET Framework provides several threading APIs that facilitate multithreading and concurrent programming. These APIs help developers manage threads, perform parallel computations, and synchronize access to shared resources. Here's an overview of the key threading APIs:

**1. System.Threading.Thread Class**

* **Purpose**: Allows you to create and manage threads explicitly.
* **Key Methods**:
  + **Start()**: Begins the execution of the thread.
  + **Join()**: Blocks the calling thread until the thread represented by this instance terminates.
  + **Sleep(int milliseconds)**: Suspends the thread for a specified duration.
* **Example**:

Thread myThread = new Thread(() =>

{

Console.WriteLine("Hello from the thread!");

});

myThread.Start();

**2. System.Threading.Tasks.Task Class**

* **Purpose**: Provides a higher-level abstraction for asynchronous and parallel programming.
* **Key Methods**:
  + **Run(Func<Task> function)**: Starts a task that runs the specified function.
  + **Wait()**: Blocks the calling thread until the task completes.
  + **ContinueWith(Func<Task, Task> continuation)**: Specifies an action to run when the task completes.
* **Example**:

Task.Run(() =>

{

Console.WriteLine("Hello from the task!");

}).Wait();

**3. System.Threading.ThreadPool Class**

* **Purpose**: Manages a pool of worker threads for executing tasks efficiently.
* **Key Methods**:
  + **QueueUserWorkItem(WaitCallback callback)**: Queues a method for execution on a thread pool thread.
  + **SetMinThreads(int workerThreads, int completionPortThreads)**: Sets the minimum number of threads in the pool.
* **Example**:

ThreadPool.QueueUserWorkItem(state =>

{

Console.WriteLine("Hello from the thread pool!");

});

**4. System.Threading.Tasks.Parallel Class**

* **Purpose**: Provides methods for parallel programming, including parallel loops and parallel queries.
* **Key Methods**:
  + **For(int from, int to, Action<int> body)**: Executes a for loop in parallel.
  + **ForEach<T>(IEnumerable<T> source, Action<T> body)**: Executes a foreach loop in parallel.
* **Example**:

Parallel.For(0, 10, i =>

{

Console.WriteLine($"Hello from iteration {i}!");

});

**5. System.Threading.Monitor Class**

* **Purpose**: Provides mechanisms for mutual exclusion and synchronization.
* **Key Methods**:
  + **Enter(object obj)**: Acquires an exclusive lock on the specified object.
  + **Exit(object obj)**: Releases the lock on the specified object.
  + **Wait(object obj)**: Blocks the current thread until it is notified.
  + **Pulse(object obj)**: Notifies a waiting thread.
* **Example**:

private static readonly object lockObject = new object();

void CriticalSection()

{

Monitor.Enter(lockObject);

try

{

Console.WriteLine("In critical section");

}

finally

{

Monitor.Exit(lockObject);

}

}

**6. System.Threading.Semaphore Class**

* **Purpose**: Controls access to a resource pool with a specified number of concurrent entries.
* **Key Methods**:
  + **WaitOne()**: Blocks the current thread until the semaphore is available.
  + **Release()**: Releases the semaphore, allowing another thread to enter.
* **Example**:

Semaphore semaphore = new Semaphore(2, 2); // Allow up to 2 concurrent entries

void AccessResource()

{

semaphore.WaitOne();

try

{

Console.WriteLine("Accessing shared resource");

}

finally

{

semaphore.Release();

}

}

**7. System.Threading.ReaderWriterLockSlim Class**

* **Purpose**: Provides a lock that allows multiple threads to read data concurrently but ensures exclusive access for writers.
* **Key Methods**:
  + **EnterReadLock()**: Acquires a read lock.
  + **EnterWriteLock()**: Acquires a write lock.
  + **ExitReadLock()**: Releases a read lock.
  + **ExitWriteLock()**: Releases a write lock.
* **Example**:

ReaderWriterLockSlim rwLock = new ReaderWriterLockSlim();

void ReadData()

{

rwLock.EnterReadLock();

try

{

Console.WriteLine("Reading data");

}

finally

{

rwLock.ExitReadLock();

}

}

void WriteData()

{

rwLock.EnterWriteLock();

try

{

Console.WriteLine("Writing data");

}

finally

{

rwLock.ExitWriteLock();

}

}

**Summary**

* **System.Threading.Thread**: Low-level control of threads.
* **System.Threading.Tasks.Task**: Higher-level abstraction for async and parallel operations.
* **System.Threading.ThreadPool**: Efficient management of worker threads.
* **System.Threading.Tasks.Parallel**: Parallel loops and queries.
* **System.Threading.Monitor**: Mutual exclusion and synchronization.
* **System.Threading.Semaphore**: Controls access to limited resources.
* **System.Threading.ReaderWriterLockSlim**: Optimized locking for read-write scenarios.

**Working of threading API for Microsoft .NET framework**

In the Microsoft .NET Framework, threading APIs provide a robust way to create, manage, and control threads. These APIs are designed to make multithreading easier and more efficient compared to traditional Win32 threading APIs. Below is an overview of how the .NET threading API works, along with an example of creating a thread and setting its priority.

**Overview of .NET Threading API**

1. **Creating Threads**:
   * The primary class for working with threads is System.Threading.Thread.
   * Threads are created by instantiating a Thread object and passing a delegate that points to the method to be executed by the thread.
2. **Starting Threads**:
   * Once a thread is created, it must be started using the Start() method. This method transitions the thread to a runnable state.
3. **Thread Priority**:
   * Threads can be assigned different priority levels using the Priority property of the Thread class.
   * The priority levels are: Highest, AboveNormal, Normal, BelowNormal, and Lowest.
4. **Stopping Threads**:
   * Threads can be stopped by letting the method finish or by using methods like Abort(), though using Abort() is not recommended for graceful termination.
5. **Waiting for Threads**:
   * The Join() method is used to block the calling thread until the thread being joined has finished execution.

**Example of Creating a Thread and Setting Its Priority**

Here is a simple example demonstrating how to create a thread, set its priority, and start it in C#:

using System;

using System.Threading;

class Program

{

// Method to be executed by the thread

static void ThreadFunc()

{

for (int i = 0; i < 5; i++)

{

Console.WriteLine("Hello from the thread!");

Thread.Sleep(1000); // Sleep for 1 second

}

}

static void Main()

{

// Create a new thread and assign it a ThreadStart delegate

Thread myThread = new Thread(new ThreadStart(ThreadFunc));

// Set the thread priority

myThread.Priority = ThreadPriority.AboveNormal;

// Start the thread

myThread.Start();

// Main thread work

for (int i = 0; i < 5; i++)

{

Console.WriteLine("Hello from the main thread!");

Thread.Sleep(500); // Sleep for 0.5 seconds

}

// Wait for the created thread to finish

myThread.Join();

Console.WriteLine("Main thread has finished.");

}

}

**Explanation**

1. **Thread Creation**:
   * A new thread is created using the Thread constructor and a delegate pointing to the ThreadFunc method.
2. **Setting Priority**:
   * The Priority property of the Thread object is set to ThreadPriority.AboveNormal, which indicates that the thread has a higher priority than normal but is not the highest priority.
3. **Starting the Thread**:
   * The Start() method is called to begin execution of the thread.
4. **Main Thread Execution**:
   * The main thread also performs some work, printing messages to the console and sleeping.
5. **Joining the Thread**:
   * The Join() method is used to ensure that the main thread waits for myThread to complete before proceeding.

By using the Thread class and its methods, you can effectively manage and control threads in your .NET applications. This approach helps in performing multiple tasks concurrently, improving the overall efficiency of the application.

Top of Form

Bottom of Form

**POSIX Threads**

POSIX Threads, also known as Pthreads, is a standard for creating and managing threads in a POSIX-compliant operating system. POSIX (Portable Operating System Interface) is a set of standards for maintaining compatibility between operating systems.

Pthreads provide a way to create multiple threads of execution within a process, allowing for concurrent execution of tasks and improving the overall performance and responsiveness of an application. The POSIX Threads standard defines a set of APIs (Application Programming Interfaces) for creating, managing, and synchronizing threads.

**Key Features of POSIX Threads:**

* **Thread Creation**: The pthread\_create() function creates a new thread, which executes a specified function.
* **Thread Synchronization**: Pthreads provide various synchronization mechanisms, such as:
  + **Mutexes (pthread\_mutex\_t)**: Mutual exclusion locks for protecting shared resources.
  + **Condition Variables (pthread\_cond\_t):** Used for signaling and waiting between threads.
  + **Semaphores (sem\_t):** Counting semaphores for controlling access to shared resources.
  + **Barriers (pthread\_barrier\_t):** These make threads wait until all of them reach a certain point before any of them can proceed.
* **Thread Management:** Pthreads provide functions for:
  + **Thread Joining**: You can use pthread\_join() to wait for a thread to finish its work before moving on.
  + **Thread Detaching**: Detaching a thread from the parent process using pthread\_detach().
  + **Thread Cancellation**: Canceling a thread using pthread\_cancel().
* **Thread-Specific Data**: Pthreads allow threads to store and retrieve thread-specific data using pthread\_setspecific() and pthread\_getspecific().

Pthreads are commonly used in:

**Server applications:** To handle multiple client connections concurrently.

**Real-time systems:** To improve responsiveness and performance.

**Scientific simulations:** To parallelize computationally intensive tasks.

**Embedded systems:** To optimize resource usage and performance.

**Common Pthread Functions**

* pthread\_create(): Creates a new thread.
* pthread\_join(): Waits for a thread to terminate.
* pthread\_exit(): Terminates the current thread.
* pthread\_mutex\_init(): Initializes a mutex (mutual exclusion) lock.
* pthread\_mutex\_lock(): Acquires a mutex lock.
* pthread\_mutex\_unlock(): Releases a mutex lock.

**Threading a Loop**

* **Concept:** Converting a loop into multiple threads so that each thread handles different iterations of the loop simultaneously.
* **Challenge:** The original order of loop iterations can change, and the loop body might not be atomic, meaning operations in different iterations could run at the same time.

**Loop-Carried Dependence**

* **Definition:** When iterations of a loop depend on each other, making it impossible to run them in parallel safely.
* **Types:**
  + **Flow Dependence:** When one iteration writes to a memory location, and a later iteration reads from that same location.
  + **Output Dependence:** Two different iterations write to the same memory location.
  + **Anti-Dependence:** When one iteration reads from a memory location before another iteration writes to it.
* **Examples:**
  + **Loop-Carried Dependence:** Iteration i writes to a location that iteration i+1 reads.
  + **Loop-Independent Dependence:** Both iterations i and i+1 access the same memory location, but within the same iteration.

**Data Race Condition**

* A data race condition occurs in parallel programming when two or more threads access shared data concurrently, and at least one of them modifies the data. This can lead to unpredictable results and bugs that are difficult to reproduce and debug.
* While OpenMP provides tools for parallel programming, it doesn't automatically detect data races.
* OpenMP compilers often ignore data race detection, relying on programmers to ensure correct synchronization.

 **Solutions:**

* **Privatization:** Using private(x) clause in OpenMP to create thread-local copies.
* **Synchronization:** Employing mutexes or other synchronization mechanisms.

 **Challenges:** Data races can be difficult to detect and reproduce.

 **Tools:** Intel® Thread Checker can assist in identifying data races.

**Managing Shared and Private Data:**

**1. Shared Data:**

* **Definition:** Data that can be accessed and modified by multiple threads.
* **Management Techniques:**
  + **Locks:** Use mutexes or spinlocks to ensure that only one thread can access the shared data at a time.
  + **Atomic Operations:** Use atomic operations for simple data types (e.g., atomic increment) to avoid the overhead of locks.
  + **Condition Variables:** Use condition variables with locks to manage complex interactions between threads.
  + **Read/Write Locks:** Use read/write locks to allow multiple threads to read shared data simultaneously while ensuring exclusive access for writes.

**2. Private Data:**

* **Definition:** Data that is local to a thread and not accessed by other threads.
* **Management Techniques:**
  + **Thread-local Storage:** Use thread-local storage (TLS) to keep data unique to each thread,so it doesn't get mixed up with data from other threads..
  + **Avoid Sharing:** Make sure private data isn't accidentally shared by avoiding global variables or shared references.
  + **Scoped Variables:** Keep variables within the function or thread where they're used, so other threads can't access them.

**Loop Scheduling and Partitioning**

* **Objective:** Achieve good performance by distributing work evenly across threads to avoid idle cores and reduce scheduling overhead.
* **Goal:** Keep all cores busy and minimize the time spent on scheduling and synchronization.

**Loop scheduling and partitioning** refer to how loop iterations are distributed among multiple threads in a parallel computing environment. The goal is to balance the workload evenly across threads to maximize performance and minimize idle time.

#### Key Concepts:

* **Scheduling Strategies:**
  + **Static Scheduling:**
    - In static scheduling, loop iterations are divided into equal-sized chunks, and each chunk is assigned to a thread before execution begins.
  + **Dynamic Scheduling:**
    - In dynamic scheduling, iterations are assigned to threads on the fly, meaning that a thread is given new iterations as soon as it finishes its current chunk.
  + **Guided Scheduling:**
    - In guided scheduling, the size of the chunks assigned to threads decreases over time. This approach starts with larger chunks and then progressively reduces the size, which helps with load balancing when later iterations take less time.
  + **Partitioning:**
    - Partitioning involves dividing the loop iterations among threads based on the chosen scheduling strategy. The effectiveness of partitioning depends on the workload distribution and the scheduling method used.

**Summary:**

* **Threading a Loop:** Runs loop iterations in parallel but requires careful handling of data dependencies.
* **Loop-Carried Dependence:** When iterations rely on each other, it’s crucial to ensure there are no dependencies before parallelizing.
* **Data Races:** Occur when multiple threads access the same data without proper control. Use synchronization to manage shared data.
* **Data Management:** OpenMP helps manage shared and private data, with private data being specific to each thread.
* **Performance:** Effective loop scheduling and partitioning are key for optimal performance in multi-threaded applications.

**Managing Shared and Private Data in OpenMP**

In OpenMP, understanding which data is shared and which is private is crucial for program correctness and performance. OpenMP provides a set of clauses, such as **shared**, **private**, and **default**, to help manage shared and private data.

# Shared Data

When memory is identified as shared, all threads access the exact same memory location. By default, all variables in a parallel region are shared, with a few exceptions.

# Private Data

When memory is identified as private, a separate copy of the variable is made for each thread to access privately. When the loop exits, these private copies become undefined.

# Privatization

Privatization is done by making a distinct copy of each variable for each thread. There are four clauses that can be used to specify privatization:

1. **private**: Each variable in the list should have a private copy made for each thread. The private copy is initialized with its default value.
2. **firstprivate**: Similar to **private**, but the private copy is initialized with the value of the variable before the parallel region.
3. **lastprivate**: Similar to **private**, but the private copy is updated with the value of the variable after the parallel region.
4. **reduction**: A reduction operation is performed on the private copies of the variable.

# Declaring Private Memory

There are three ways to declare private memory in OpenMP:

1. Use the **private**, **firstprivate**, **lastprivate**, or **reduction** clause to specify variables that need to be private for each thread.
2. Use the **threadprivate** pragma to specify global variables that need to be private for each thread.
3. Declare the variable inside the loop, without the **static** keyword, within the OpenMP parallel region.

**Directory-based cache coherence protocol**

The directory-based cache coherence protocol is a popular approach to implement distributed shared memory (DSM) architecture in multiprocessor systems. Here's an explanation of how it works:

**Overview**

In a DSM system, multiple processors or nodes share a common memory space, and each node has its own cache to store frequently accessed data. The directory-based cache coherence protocol ensures that the caches remain consistent across all nodes, even in the presence of concurrent updates.

**Directory Structure**

The directory is a centralized data structure that keeps track of the cache coherence information for each memory block. The directory is typically implemented as a table or array, where each entry corresponds to a memory block. Each entry contains the following information:

1. **Block ID**: Unique identifier for the memory block.
2. **Node ID**: ID of the node that currently owns the block (i.e., has the most up-to-date copy).
3. **Cache State**: Indicates the cache state of the block on each node (e.g., valid, invalid, shared, exclusive).
4. **Sharers List**: List of nodes that currently have a shared copy of the block.

**Protocol Operation**

Here's a step-by-step explanation of how the directory-based cache coherence protocol works:

1. **Read Request**: When a node needs to access a memory block, it sends a read request to the directory.
2. **Directory Lookup**: The directory checks its table to determine the current owner of the block and its cache state.
3. **Cache Hit**: If the requesting node already has a valid copy of the block in its cache, the directory returns a cache hit response, and the node can access the block locally.
4. **Cache Miss**: If the requesting node does not have a valid copy, the directory sends a cache miss response, indicating the current owner of the block.
5. **Block Transfer**: The requesting node sends a request to the current owner node to transfer the block. The owner node responds with the block data and updates its cache state to "shared".
6. **Cache Update**: The requesting node updates its cache with the received block data and sets its cache state to "shared".
7. **Sharers List Update**: The directory updates the sharers list to include the requesting node.
8. **Write Request**: When a node needs to update a memory block, it sends a write request to the directory.
9. **Invalidation**: The directory sends an invalidation message to all nodes in the sharers list, indicating that their cached copies are no longer valid.
10. **Block Update**: The writing node updates the block data and sets its cache state to "exclusive".
11. **Directory Update**: The directory updates the block ID, node ID, and cache state information.

**Advantages**

The directory-based cache coherence protocol offers several advantages, including:

* **Scalability**: The protocol can handle a large number of nodes and memory blocks.
* **Flexibility**: It supports various cache coherence policies, such as MESI (Modified, Exclusive, Shared, Invalid) or MOESI (Modified, Owned, Exclusive, Shared, Invalid).
* **Low Latency**: The protocol minimizes latency by reducing the number of messages exchanged between nodes.

**Challenges**

While the directory-based cache coherence protocol is effective, it also presents some challenges, such as:

* **Directory Bottleneck**: The directory can become a bottleneck as the number of nodes and memory blocks increases.
* **Cache Coherence Traffic**: The protocol generates additional traffic due to cache coherence messages, which can impact system performance.

**Current IA-32 Architecture**

**IA-32** is a type of computer design from a time when computers had only one processor. It was designed to be fast and still work with old programs.

#### Key Points:

1. **Consistency vs. Speed**:
   * **Sequential Consistency**: This means all the actions (like reading and writing data) by different parts of a program should appear in a fixed order. If computers strictly followed this, they would be slower.
   * **IA-32 Approach**: It makes some changes to speed things up but still tries to avoid breaking old programs.
2. **Two Main Rules**:
   * **Flexibility for Speed**:
     + Threads (parts of a program running at the same time) might read data from their own fast memory instead of waiting for the main memory, but this doesn’t always affect the order in which they see data.
   * **Strictness for Safety**:
     + Special commands (like the LOCK prefix) make sure that important operations happen in the correct order so that things work correctly, especially when different parts of the program need to coordinate.
3. **What It Means for Old Algorithms**:
   * **Processor Order**: IA-32 allows some flexibility in the order of operations to improve speed but fixes problems if it causes issues.
   * **Old Algorithms**: Some old methods for ensuring only one part of a program runs at a time (like Dekker’s Algorithm) might not work as expected on IA-32 because of this flexibility.

**In Short**: IA-32 tries to be quick and compatible with old software. However, its way of managing memory order can sometimes cause problems with older methods that assume a strict order of operations.

**Methods to Avoid Pipeline Stalls in IA-32 (Simplified)**

1. **Out-of-Order Execution**: The processor can execute instructions out of their original order, depending on when the needed data is ready. This helps keep the pipeline busy and reduces waiting time.
2. **Branch Prediction**: The processor guesses the direction a branch (like an "if" statement) will take and starts executing those instructions ahead of time. If the guess is correct, it avoids delays.
3. **Speculative Execution**: The processor begins working on instructions before it's certain they are needed, based on predictions. If the predictions are correct, this saves time.
4. **Register Renaming**: The processor avoids unnecessary waiting by assigning temporary registers to instructions. This prevents "fake" dependencies between instructions that use the same register.
5. **Superscalar Execution**: The processor can handle multiple instructions at the same time, which helps speed up processing and avoids delays in the pipeline.

**cache line ping-ponging**

* Non-blocking algorithms can cause a lot of traffic on the memory bus because multiple threads are trying to access the same data at the same time.
* This can lead to a situation where the data is constantly being passed back and forth between threads, like a game of ping-pong.
* In some cases, using a locked algorithm (where one thread has exclusive access to the data) might be faster than a non-blocking algorithm.
* This is because the locked algorithm can say "wait, I'm not done with this data yet" and prevent other threads from accessing it.
* To figure out which approach is better, you need to experiment and test both options.
* A general rule of thumb is that if a locked algorithm is protecting a small section of code with no atomic operations, it might be faster than a non-blocking algorithm that requires multiple atomic operations.

**False Sharing:**

* False sharing occurs when multiple threads access different variables that happen to be located in the same cache line.
* Even though the threads are accessing different variables, the cache line is still shared between them.
* When one thread modifies its variable, the entire cache line is marked as dirty and must be updated, which can cause other threads to reload the cache line unnecessarily.
* This can lead to performance degradation due to increased cache misses and memory traffic.

|  |  |  |
| --- | --- | --- |
| Characteristic | False Sharing | Cache Line Ping-Ponging |
| Access Pattern | Multiple threads access different variables in the same cache line | Multiple threads access the same cache line, often due to a shared variable or lock |
| Cache Line Updates | Entire cache line is marked as dirty and updated when one thread modifies its variable | Cache line is sent back and forth between threads, with each thread modifying it |
| Performance Impact | Increased cache misses, memory traffic, and performance degradation | High volume of cache line transfers, leading to performance degradation and increased memory traffic |
| Cause | Poor data layout or alignment | Contention for a shared resource, such as a lock or shared variable |
| Solution | Improve data layout, use padding or alignment to separate variables | Use locks or other synchronization mechanisms to reduce contention, or consider non-blocking algorithms |

**Memory Consistency**

**Sequential Consistency:**

* **What It Means:**
  + In a single-threaded program, memory operations happen in a predictable order, so the memory always has a well-defined state at any point in time. This is known as sequential consistency.

**Parallel Programs:**

* **Issue with Memory Order:**
  + In parallel programs, where multiple threads or processors are working simultaneously, the order in which memory operations are seen can vary. This happens because:
    - **Buffers and Caches:** When a thread writes data, it first goes to buffers and caches before reaching the main memory. A later write might reach the main memory before an earlier write due to these delays.
    - **Read and Write Order:** A later read that hits the cache might finish before an earlier read that needs to fetch from the main memory.

**Consistency in Parallel Programs:**

* **Relaxed Consistency:**
  + In parallel systems, the order in which one thread sees the actions of another thread might not be the same as the order in which they were executed. This is called relaxed consistency.
  + **Self-Consistency:** Each thread sees its own operations in the correct order, but might not see other threads' operations in the same order.

**Impact on Programs:**

* **Single-threaded vs. Multi-threaded:**
  + On single-threaded systems or systems with simple hardware threading (like hyper-threading), consistency issues might not be noticeable. But on more complex multi-threaded systems with separate caches, programs can fail if they don’t handle consistency properly.

**OpenMP Runtime Library Routines**

### Controlling Parallelism

* **omp\_set\_num\_threads(num\_threads):**
  + Sets the number of threads to be used in subsequent parallel regions.
  + num\_threads is an integer specifying the desired number of threads.
* **omp\_get\_num\_procs():**
  + Returns the number of processors available to the program.
  + Useful for determining the maximum potential number of threads.
* **omp\_get\_dynamic():**
  + Returns a logical value indicating whether the number of threads can be dynamically adjusted at runtime.
  + True if dynamic adjustment is enabled, False otherwise.
* **omp\_get\_nested():**
  + Returns a logical value indicating whether nested parallelism is enabled.
  + True if nested parallelism is allowed, False otherwise.

### Synchronization

* **omp\_unset\_lock(lock):**
  + Releases a previously acquired lock.
  + lock is an integer variable of type omp\_lock\_kind used to identify the lock.

### Timing

* **omp\_get\_wtick():**
  + Returns the time resolution of the system clock in seconds.
  + Useful for calculating elapsed time with higher precision.
* **omp\_get\_wtime():**
  + Returns the current wall-clock time in seconds.
  + Commonly used to measure elapsed time between events.

## OpenMP Library Functions and Environment Variables

### (i) OpenMP Library Functions

OpenMP provides a set of library functions that can be used to control the execution of parallel regions and manage thread-related information. Here are some commonly used functions:

* **omp\_get\_num\_threads():** Returns the number of threads in the current parallel region.
* **omp\_get\_thread\_num():** Returns the thread ID within the current parallel region.
* **omp\_set\_num\_threads():** Sets the number of threads to be used in subsequent parallel regions.
* **omp\_get\_max\_threads():** Returns the maximum number of threads supported by the OpenMP implementation.
* **omp\_in\_parallel():** Returns a boolean value indicating whether the current thread is within a parallel region.
* **omp\_get\_wtime():** Returns the elapsed wall-clock time since the program started.
* **omp\_get\_thread\_num():** Returns the thread ID within the current parallel region.

### (ii) OpenMP Environment Variables

OpenMP also supports a set of environment variables that can be used to configure the runtime behavior of the library. Some commonly used environment variables include:

* **OMP\_NUM\_THREADS:** Sets the default number of threads to be used in parallel regions.
* **OMP\_SCHEDULE:** Specifies the scheduling policy for parallel loops (e.g., static, dynamic, guided).
* **OMP\_NESTED:** Controls whether nested parallelism is enabled.
* **OMP\_WAIT\_POLICY:** Specifies the waiting policy for parallel regions (e.g., active, passive).
* **OMP\_STACKSIZE:** Sets the stack size for threads.

**Data Parallelism in OpenMP**

* **Data Decomposition:** The data to be processed is divided into smaller chunks, and each chunk is assigned to a different thread.
* **Parallel Loops:** #pragma omp parallel for is the primary construct for data parallelism. It automatically distributes iterations of a loop among threads.
* **Synchronization:** OpenMP provides synchronization mechanisms like critical, atomic, and barrier to coordinate access to shared data and ensure correct execution.

**Functional Parallelism in OpenMP**

* **Task Parallelism:** Tasks (functions or procedures) are executed in parallel.
* **Task-Based Programming:** #pragma omp task is used to define tasks that can be executed concurrently.
* **Dependency Analysis:** OpenMP can automatically analyze dependencies between tasks to ensure correct execution order.

**Loop Scheduling and Portioning in OpenMP**

In OpenMP, loop scheduling and portioning are techniques used to distribute the iterations of a loop among multiple threads, allowing for parallel execution and improved performance.

**Loop Scheduling**

Loop scheduling refers to the process of dividing the iterations of a loop into smaller chunks, called **schedule units**, and assigning them to different threads for execution. The goal is to balance the workload among threads, minimize synchronization overhead, and maximize parallelism.

OpenMP provides several loop scheduling strategies, which can be specified using the **schedule** clause:

1. **Static Scheduling**: Each thread is assigned a fixed number of iterations, and the iterations are divided evenly among threads.
2. **Dynamic Scheduling**: Iterations are assigned to threads dynamically, as they become available. This strategy is useful when the iterations have varying execution times.
3. **Guided Scheduling**: A combination of static and dynamic scheduling. The iterations are divided into smaller chunks, and each thread is assigned a chunk. As threads complete their chunks, they are assigned new ones.
4. **Auto Scheduling**: The OpenMP runtime environment determines the best scheduling strategy based on the loop characteristics and system resources.

**Loop Portioning**

Loop portioning is the process of dividing the iterations of a loop into smaller, contiguous blocks, called **chunks**, and assigning them to different threads for execution. The goal is to minimize synchronization overhead and maximize parallelism.

OpenMP provides two loop portioning strategies:

1. **Block Portioning**: The iterations are divided into fixed-size blocks, and each thread is assigned a block.
2. **Cyclic Portioning**: The iterations are divided into blocks, and each thread is assigned a block in a cyclic manner (e.g., thread 0 gets iterations 0, 3, 6, ..., thread 1 gets iterations 1, 4, 7, ..., etc.).

**Data Copy-In and Copy-Out in Parallel Programming**

When parallelizing a program, you often need to manage how data is shared and copied between threads. OpenMP provides specific tools for this, called clauses, which help handle data correctly. Here's a simple breakdown:

**OpenMP Clauses for Data Copy**

1. **firstprivate**:
   * **What It Does:** Initializes each thread's private copy of a variable with the value from the master thread.
   * **When to Use:** Use this when each thread needs to start with the same value as the master thread’s variable.
2. **lastprivate**:
   * **What It Does:** Copies the final value of a variable from the last part of the parallel section back to the master thread’s variable.
   * **When to Use:** Use this if you want the master thread to have the final value of a variable after the parallel operations are done.
3. **copyin**:
   * **What It Does:** Copies a variable’s value from the master thread to all other threads in the team.
   * **When to Use:** Use this for threadprivate variables that need to be initialized with the master thread’s value at the start of the parallel section.
4. **copyprivate**:
   * **What It Does:** Shares a variable’s value from one thread with all other threads in the team.
   * **When to Use:** Use this if one thread calculates a value and you want all other threads to use this value.

**OpenMP** is a tool that helps manage this process. It has special commands to:

* **firstprivate:** Give each worker (thread) a copy of the starting data.
* **lastprivate:** Take the final result from one worker and share it with everyone.
* **copyin:** Share data among all workers at the start.
* **copyprivate:** Share data among all workers at some point during the work.

**Work-Sharing in OpenMP**

OpenMP has a feature called work-sharing that helps divide tasks among threads in a team. This example shows how to use work-sharing for loops and sections together in a single parallel region.

**How it Works**

1. OpenMP creates a team of threads.
2. The loop iterations are divided among the threads.
3. Once the loop is finished, the sections are divided among the threads.
4. Each section is executed exactly once, but in parallel with the other sections.
5. If there are more sections than threads, the remaining sections are scheduled as threads finish their previous sections.